{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Expectations","CC SC-Agreement","Measurement Method Details","(Equipment Name)_Setup","X-Ray_Setup Example1","Pull Strength_Setup Example2","Information"],"not_rendered":{"charts":0,"images":11,"macros":0,"external_links":0,"defined_names":5,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Expectations","index":0,"n_rows":28,"n_cols":1,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["General expectations for PPAP and serial inspections"]
["(Explanation for measurement agreements)"]
[]
["Instruction"]
["If not otherwise specified supplier shall fill the drawing information and propose the measurement for PPAP presentation and serial inspection. "]
["Veoneer SQ and Design Engineer needs to verify and approve the measurement agreement. "]
[]
["Alignment"]
["Use alignment described in drawing and confirm in PPAP that it was applied."]
["If alignment is not defined on drawing, agree method with Veoneer SQ and Design Engineer during APQP."]
[]
["Measurement"]
["In general the measuring method shall correspond to the function of the measured dimension. Some Special Characteristics require specific measurement methods and points. These methods needs to be agreed with the Veoneer SQ & Design Engineer during APQP. The measurement methode has to be in correlation between Supplier and Veoneer. "]
[]
["Initial Process Studies (IPS)"]
["IPS is required for all CC, SC and SPC dimensions."]
["The purpose of IPS is to understand the process variation, not just to achieve a specific index value. Ppk should be calculated from at least 100 individual samples."]
[" =< Deviations from above regulation require measurement agreement proposed by supplier during APQP. "]
["Before IPS is performed MSA shall be proven acceptable. "]
[]
["Measurement System Analysis (MSA)"]
["All measurement methods used to verify CC and SC dimensions, applicable MSA must be included in PPAP."]
["Target: GR&R less than 10% = acceptable; "]
["GR&R 11%-20% = acceptable, but need for improvement plan; "]
["GR&R above 21%= not acceptable need for corrective action plan"]
[]
["Serial inspection"]
["Even if agreement was made to waive Cpk observation during serial inspection, values have to be documented and must be proven capable when analyzed."]

{"sheet":"CC SC-Agreement","index":1,"n_rows":44,"n_cols":19,"rows_kept":44,"cut":false,"hidden":false,"merged":[[43,0,43,14],[42,0,42,14],[23,0,23,14],[24,0,24,14],[25,0,25,14],[26,0,26,14],[22,0,22,14],[39,0,39,14],[40,0,40,14],[41,0,41,14],[20,1,20,14],[0,3,0,7],[1,3,1,7],[2,3,2,5],[3,3,3,7],[0,11,0,14],[1,11,1,12],[2,11,2,12],[3,11,3,12]]}
[null,null,"Supplier:",null,null,null,null,null,null,"Date (Orig.):"]
[null,null,"Part Name:",null,null,null,null,null,null,"Date (Update):",null,null,null,"ECL:"]
[null,null,"Drawing Number:",null,null,null,"ECL:",null,null,"Date (Update):",null,null,null,"ECL:"]
["Measurement Agreement",null,"Part Number:",null,null,null,null,null,null,"Date (Update):",null,null,null,"ECL:"]
["Dimensions"]
["Drawing information",null,null,"Measurements/Verification for PPAP",null,null,null,null,"Control in serial production"]
["Pos.","[CC] / [SC] ?","Dimension/\nTolerance","Measurement method","MSA [X if required]","Details for measurement","Sample Size","IPS\n[x if req. or target Ppk]","Measurement Method","MSA [X if required]","Details for measurement\n[as defined for PPAP, unless otherwise defined]","Sample Size","Frequency","Observe Cpk\n[x if req.]","Comments","reference MSA","reference IPS","estimate Ppk\n[x if req.]","Submit measured samples with PPAP"]
["All, unless mentioned below",null,"Annual layout according to specification/ drawing","Various",null,null,"1/cav.",null,"Various",null,null,"1/cav.","Annual",null,"Date for annual layout to be defined in Control Plan"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Remarks:","Abbreviations: CMM=Coordinate Measurement Machine; DR=Dimensional Repor; ref.=reference plane or line; req.=requested; SOP=start of production order; IPS=Initial process study; MSA=Measurement System Analysis; VSM=Veoneer Supplier Manual."]
[]
["VSM (Veoneer Supplier Manual) applies independent of this agreement. With this agreement Veoneer defines minimum requirements."]
["All process specific/Special characteristics and other additional positions required by the process flow and / or P-FMEA have to be added in the control plan by the supplier independently."]
["This Measurement Agreement is valid without update to new drawing revisions if content is unaffected and no need for update has been identified. Veoneer can recall this agreement at any time."]
["The Measurement Agreement is based on proposal and P-FMEA evaluation of supplier. Veoneer acceptance is based on experience and trust in suppliers know how and risk evaluation."]
["Supplier remains fully responsible for any dimensional deviations not approved by Veoneer in PPAP and their effects even if Veoneer accepted reduced measuring frequency or waived IPS."]
[]
[]
[]
["(Print and Sign Name)",null,"Veoneer Design Engineer",null,null,"Date",null,null,"(Print and Sign Name)",null,"Supplier Quality Manager",null,null,null,"Date"]
[]
[]
[]
[]
["(Print and Sign Name)",null,"Veoneer Supplier Quality",null,null,"Date",null,null,"(Print and Sign Name)",null,"Supplier  (Title)",null,null,null,"Date"]
[]
[]
[]
["VSM (Veoneer Supplier Manual) applies independent of this agreement. With this agreement Veoneer defines minimum requirements."]
["All process specific/Special characteristics and other additional positions required by the process flow and / or P-FMEA have to be added in the control plan by the supplier independently."]
["This Measurement Agreement is valid without update to new drawing revisions if content is unaffected and no need for update has been identified. Veoneer can recall this agreement at any time."]
["The Measurement Agreement is based on proposal and P-FMEA evaluation of supplier. Veoneer acceptance is based on experience and trust in suppliers know how and risk evaluation."]
["Supplier remains fully responsible for any dimensional deviations not approved by Veoneer in PPAP and their effects even if Veoneer accepted reduced measuring frequency or waived IPS."]

{"sheet":"Measurement Method Details","index":2,"n_rows":2,"n_cols":7,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["The Measurement Method of the Datum"]
["NO.","Drawing NO.","Dimension","   Measurement the datum.                    ","Position of the drawing\n[Drawing Element(s) Capture(s)]","   Measurement method\n(Details, Drawings, Images)                                                             ","Equipment / Tool"]

{"sheet":"(Equipment Name)_Setup","index":3,"n_rows":61,"n_cols":15,"rows_kept":61,"cut":false,"hidden":false,"merged":[[4,6,18,6],[1,0,1,20],[19,6,33,6],[38,0,38,7],[60,0,63,9],[60,11,63,20],[38,11,38,20],[19,14,33,20],[4,14,18,20],[4,7,18,13],[19,7,32,13],[3,14,3,20],[3,7,3,13]]}
["Note:  Repeat this worksheet for additional equipment."]
["<Insert Equipment Name / Process>"]
["Test Items："]
[null,null,null,null,null,null,"Step","Test Introduction",null,null,null,null,null,null,"Sketch / Image"]
[null,null,"Equipment Picture"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes:"]
[]
[]
[]
["<Insert Data / Graph / Image Title>",null,null,null,null,null,null,null,null,null,null,"<Insert Data / Graph / Image Title>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes:",null,null,null,null,null,null,null,null,null,null,"Description / Notes:"]

{"sheet":"X-Ray_Setup Example1","index":4,"n_rows":75,"n_cols":15,"rows_kept":75,"cut":false,"hidden":false,"merged":[[0,0,0,20],[1,0,2,5],[2,7,2,13],[2,14,2,20],[3,6,17,6],[3,7,17,13],[3,14,17,20],[52,0,52,6],[52,11,52,20],[74,11,77,20],[18,6,32,6],[18,7,32,13],[18,14,32,20],[33,6,47,6],[33,7,46,13],[33,14,47,20]]}
["Alloy Composition Analysis Machine (X-Ray) - EXAMPLE 1"]
["Test Items：Alloy composition analysis"]
[null,null,null,null,null,null,"Step","Test Introduction",null,null,null,null,null,null,"Sketch / Image"]
["Equipment Picture",null,null,null,null,null,"1. Calibration","Use Ag calibration part to calibrate the equipment:\n1. Place the Ag calibration part in the centre of test area and then close the cover.\n2. click the calibration button to start, when it is done, 'Calibration completed' will be showing in the screen.\n\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"2. Place the test specimen in the test area and then run the test","1. Open the cover and place the test specimen in the test area.\n2. Choose the test profile. Select test type of \"composition analysis of solder alloy\", and then start the test.\n\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"NAYUR-1000"]
[]
[]
[]
[null,null,null,null,null,null,"3. Testing result reporting","when test is completed, test results will be showing in the screen as the picture on the right.\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes:"]
[]
[]
[]
["Test report"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"`"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes:"]

{"sheet":"Pull Strength_Setup Example2","index":5,"n_rows":60,"n_cols":15,"rows_kept":60,"cut":false,"hidden":false,"merged":[[59,0,62,9],[59,11,62,20],[0,0,0,20],[2,7,2,13],[2,14,2,20],[3,6,17,6],[3,7,17,13],[3,14,17,20],[18,6,32,6],[18,7,31,13],[18,14,32,20],[37,0,37,7],[37,11,37,20]]}
["Pull Strength Tester - Example2"]
["Test Items：Adhesion force test for lens-assembly"]
[null,null,null,null,null,null,"Step","Test Introduction",null,null,null,null,null,null,"Sketch / Image"]
[null,null,"Equipment Picture",null,null,null,1,"Zeroing the gauge, and then install the lens-assembly specimen between upper-clamp and lower-clamp fixture."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,2,"Press Test button to start the test, when test completes, record the pull strength force value shown in the display. "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes:"]
[]
[]
[]
["<Insert Data / Graph / Image Title>",null,null,null,null,null,null,null,null,null,null,"<Insert Data / Graph / Image Title>"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Description / Notes: Adhesion force population",null,null,null,null,null,null,null,null,null,null,"Description / Notes:"]

{"sheet":"Information","index":6,"n_rows":3,"n_cols":5,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Version #","Date","Author","Modification","Purpose"]
[1,"2020-04-01","Dennis Nielsen","New Release"]
[1.1000000000000001,"2022-06-14","Jose Dorado","Update to CC-SC Agreement - add \"Veoneer\"","Clarification"]